location:
  type: auto # or static
  # latitude: 45.4215
  # longitude: -75.6972
  # provider: CA # Optional: force US or CA

language: en # Options: en, fr

voice:
  # Example utilizing pico2wave (sudo apt install libttspico-utils)
  # {lang} is replaced by 'en-US' or 'fr-FR'
  tts_command: 'pico2wave -l {lang} -w /tmp/temp.wav "{text}" && sox /tmp/temp.wav -r 8000 -c 1 {file}'

audio:
  nodes: 
    - "YOUR_NODE_NUMBER_HERE"

alerts:
  check_interval_minutes: 10
  min_severity: "Watch"
  # Optional: List of NWS Zones/Counties to monitor in addition to current location
  # extra_zones:
  #   - "VAC001"
  #   - "MDZ013"
