#Fox 1 Telemetry Decoder Properties
#Sat Apr 11 13:20:20 EST 2020
#File named .dat should be in the logfiles directory and is loaded by FoxTelem
#File named .MASTER should not be edited and is a backup copy in the installation directory 
foxId=7
displayName=CubeSatSim-FSK
name=CubeSatSim
model=0
IHU_SN=7
catalogNumber=0
description=CubeSatSim, the AMSAT CubeSat Simulator, is a functional satellite model that generates real telemetry from solar panels, batteries, and temperature sensors.  Use this for DUV FSK telemetry. For more information see http://cubesatsim.org
BATTERY_CURRENT_ZERO=-1.839
EXP1=0
EXP2=0
EXP3=0
EXP4=0
numberOfLayouts=4
layout0.filename=FOX1A_debug.csv
layout0.name=DEBUG
layout1.filename=FOX1A_maxtelemetry.csv
layout1.name=maxtelemetry
layout2.filename=CubeSatSim_rttelemetryFM.csv
layout2.name=rttelemetry
layout3.filename=FOX1A_mintelemetry.csv
layout3.name=mintelemetry
#layout4.filename=FOX1A_radtelemetry.csv
#layout4.name=radtelemetry
#layout5.filename=FOX1A_radtelemetry2.csv
#layout5.name=radtelemetry2
#layout5.parentLayout=radtelemetry
lookupTable0.filename=FOX1A_rssiFM.tab
numberOfLookupTables=3
lookupTable0=RSSI
lookupTable1.filename=FOX1A_ihuVBattSN7.tab
lookupTable1=IHU_VBATT
lookupTable2.filename=FOX1A_ihutempSN7.tab
lookupTable2=IHU_TEMP
telemetryDownlinkFreqkHz=434900	
maxFreqBoundkHz=434950
minFreqBoundkHz=434850
measurementsFileName=measurements.csv
memsRestValueX=2087
memsRestValueY=2101
memsRestValueZ=2045
passMeasurementsFileName=passmeasurements.csv
numberOfSources=1
source0.name=ihu.duv
#source1.name=ihu.highspeed
track=true
useIHUVBatt=true
user_mode=0
user_format=0
useConversionCoeffs=true
conversionCurvesFileName=cubesatsim_conversion_curves.csv
