(export (version D)
  (design
    (source "C:\\Users\\ajohns71\\Dropbox\\Nova\\KiCad PCB for GitHub\\cubesatsim_solar.sch")
    (date "12/15/2018 11:14:08 AM")
    (tool "Eeschema (5.0.1)-4")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "AMSAT CubeSat Simulator Solar Panel Board")
        (company)
        (rev B1.1)
        (date "December 13, 2018")
        (source cubesatsim_solar.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref D1)
      (value 1N5817)
      (footprint Diode_THT:D_DO-41_SOD81_P3.81mm_Vertical_AnodeUp)
      (datasheet ~)
      (libsource (lib pihat_template-rescue) (part D-device) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF2DDAE))
    (comp (ref J7)
      (value "INA219 Sensor Board")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib pihat_template-rescue) (part Conn_01x06_Female-Connector) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF2E1F2))
    (comp (ref J1)
      (value "Sensor Inputs")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib pihat_template-rescue) (part Conn_01x10_Female-Connector) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF2F696))
    (comp (ref J5)
      (value "RBF Switch")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical)
      (libsource (lib pihat_template-rescue) (part CONN_01X05-conn2) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF5F60C))
    (comp (ref J3)
      (value "Vdc In")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (libsource (lib pihat_template-rescue) (part CONN_01X02-conn2) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF6082F))
    (comp (ref J4)
      (value "Vout to MoPOWER")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (libsource (lib pihat_template-rescue) (part CONN_01X02-conn2) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF6089F))
    (comp (ref J2)
      (value "Battery In/Out")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (libsource (lib pihat_template-rescue) (part CONN_01X02_FEMALE-conn2) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF6F85F))
    (comp (ref P3)
      (value "GPIO Male Extra Long (19mm) 20x2 Header Pins")
      (footprint w_conn_strip:vasch_strip_20x2)
      (fields
        (field (name "Mouser Part No.") 517-30340-6002))
      (libsource (lib pihat_template-rescue) (part Raspberry_Pi_+_Conn-pihat_template-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 54E92361))
    (comp (ref R2)
      (value 4.7k)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P5.08mm_Vertical)
      (fields
        (field (name Family) Passive)
        (field (name Part) -))
      (libsource (lib pihat_template-rescue) (part RESISTOR-passive) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF91C4F))
    (comp (ref R1)
      (value 4.7k)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P5.08mm_Vertical)
      (fields
        (field (name Family) Passive)
        (field (name Part) -))
      (libsource (lib pihat_template-rescue) (part RESISTOR-passive) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF91CF1))
    (comp (ref J10)
      (value "INA219 Sensor Board")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib pihat_template-rescue) (part Conn_01x06_Female-Connector) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF9E342))
    (comp (ref J8)
      (value "INA219 Sensor Board")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib pihat_template-rescue) (part Conn_01x06_Female-Connector) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFB9855))
    (comp (ref J9)
      (value "INA219 Sensor Board")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib pihat_template-rescue) (part Conn_01x06_Female-Connector) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFBC218))
    (comp (ref J11)
      (value "INA219 Sensor Board")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib pihat_template-rescue) (part Conn_01x06_Female-Connector) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFBED5A))
    (comp (ref J12)
      (value "INA219 Sensor Board")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib pihat_template-rescue) (part Conn_01x06_Female-Connector) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFC1EC2))
    (comp (ref D2)
      (value 1N5817)
      (footprint Diode_THT:D_DO-41_SOD81_P3.81mm_Vertical_AnodeUp)
      (datasheet ~)
      (libsource (lib pihat_template-rescue) (part D-device) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFCE14D))
    (comp (ref D3)
      (value 1N5817)
      (footprint Diode_THT:D_DO-41_SOD81_P3.81mm_Vertical_AnodeUp)
      (datasheet ~)
      (libsource (lib pihat_template-rescue) (part D-device) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFD1A73))
    (comp (ref D4)
      (value 1N5817)
      (footprint Diode_THT:D_DO-41_SOD81_P3.81mm_Vertical_AnodeUp)
      (datasheet ~)
      (libsource (lib pihat_template-rescue) (part D-device) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFD565A))
    (comp (ref D5)
      (value 1N5817)
      (footprint Diode_THT:D_DO-41_SOD81_P3.81mm_Vertical_AnodeUp)
      (datasheet ~)
      (libsource (lib pihat_template-rescue) (part D-device) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFD9541))
    (comp (ref J6)
      (value "Expansion Interface")
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x05_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib pihat_template-rescue) (part Conn_01x05_Female-Connector) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFF9AD8))
    (comp (ref J13)
      (value IN+)
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical)
      (libsource (lib pihat_template-rescue) (part CONN_01X01-conn2) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C0D6034))
    (comp (ref J14)
      (value IN-)
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical)
      (libsource (lib pihat_template-rescue) (part CONN_01X01-conn2) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C0D608E))
    (comp (ref J15)
      (value OUT+)
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical)
      (libsource (lib pihat_template-rescue) (part CONN_01X01-conn2) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C0D60E4))
    (comp (ref J16)
      (value OUT-)
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical)
      (libsource (lib pihat_template-rescue) (part CONN_01X01-conn2) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C0D6176)))
  (libparts
    (libpart (lib pihat_template-rescue) (part CONN_01X01-conn2)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X01-conn2))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib pihat_template-rescue) (part CONN_01X02-conn2)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X02-conn2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib pihat_template-rescue) (part CONN_01X02_FEMALE-conn2)
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X02_FEMALE-conn2))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib pihat_template-rescue) (part CONN_01X05-conn2)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X05-conn2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))))
    (libpart (lib pihat_template-rescue) (part Conn_01x05_Female-Connector)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x05_Female-Connector))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))))
    (libpart (lib pihat_template-rescue) (part Conn_01x06_Female-Connector)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x06_Female-Connector))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))))
    (libpart (lib pihat_template-rescue) (part Conn_01x10_Female-Connector)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x10_Female-Connector))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))))
    (libpart (lib pihat_template-rescue) (part D-device)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D-device))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib pihat_template-rescue) (part RESISTOR-passive)
      (footprints
        (fp R-0603)
        (fp R-0805)
        (fp R-1206)
        (fp R-1210))
      (fields
        (field (name Reference) R)
        (field (name Value) RESISTOR-passive)
        (field (name Part) -)
        (field (name Family) Passive))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib pihat_template-rescue) (part Raspberry_Pi_+_Conn-pihat_template-rescue)
      (fields
        (field (name Reference) P)
        (field (name Value) Raspberry_Pi_+_Conn-pihat_template-rescue))
      (pins
        (pin (num 1) (name "VDD_(3.3v)") (type input))
        (pin (num 2) (name "VPP_(5v)") (type input))
        (pin (num 3) (name GPIO2/I2C1_SDA) (type input))
        (pin (num 4) (name "VPP_(5v)") (type input))
        (pin (num 5) (name GPIO3/I2C1_SCL) (type input))
        (pin (num 6) (name GND) (type input))
        (pin (num 7) (name GPIO4/GPCLK0) (type input))
        (pin (num 8) (name GPIO14/UART_TXD) (type input))
        (pin (num 9) (name GND) (type input))
        (pin (num 10) (name GPIO15/UART_RXD) (type input))
        (pin (num 11) (name GPIO17) (type input))
        (pin (num 12) (name GPIO18) (type input))
        (pin (num 13) (name GPIO27) (type input))
        (pin (num 14) (name GND) (type input))
        (pin (num 15) (name GPIO22) (type input))
        (pin (num 16) (name GPIO23) (type input))
        (pin (num 17) (name "VDD_(3.3V)") (type input))
        (pin (num 18) (name GPIO24) (type input))
        (pin (num 19) (name GPIO10/SPI_M0SI) (type input))
        (pin (num 20) (name GND) (type input))
        (pin (num 21) (name GPIO9/SPI_MISO) (type input))
        (pin (num 22) (name GPIO25) (type input))
        (pin (num 23) (name GPIO11/SPI_SCLK) (type input))
        (pin (num 24) (name GPIO8/SPI_CE0) (type input))
        (pin (num 25) (name GND) (type input))
        (pin (num 26) (name GPIO7/SPI_CE1) (type input))
        (pin (num 27) (name ID_SD) (type input))
        (pin (num 28) (name ID_SC) (type input))
        (pin (num 29) (name GPIO5) (type input))
        (pin (num 30) (name GND) (type input))
        (pin (num 31) (name GPIO6) (type input))
        (pin (num 32) (name GPIO12) (type input))
        (pin (num 33) (name GPIO13) (type input))
        (pin (num 34) (name GND) (type input))
        (pin (num 35) (name GPIO19) (type input))
        (pin (num 36) (name GPIO16) (type input))
        (pin (num 37) (name GPIO20) (type input))
        (pin (num 39) (name GND) (type input))
        (pin (num 40) (name GPIO21) (type input)))))
  (libraries
    (library (logical pihat_template-rescue)
      (uri "C:\\Users\\ajohns71\\Dropbox\\Nova\\KiCad PCB for GitHub/pihat_template-rescue.lib")))
  (nets
    (net (code 1) (name Y+In)
      (node (ref J8) (pin 1))
      (node (ref J1) (pin 3)))
    (net (code 2) (name +3V3)
      (node (ref J11) (pin 6))
      (node (ref J12) (pin 6))
      (node (ref J10) (pin 6))
      (node (ref R2) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref J7) (pin 6))
      (node (ref J8) (pin 6))
      (node (ref P3) (pin 1))
      (node (ref J6) (pin 2))
      (node (ref J9) (pin 6)))
    (net (code 3) (name GND)
      (node (ref J3) (pin 2))
      (node (ref J4) (pin 2))
      (node (ref J12) (pin 5))
      (node (ref J1) (pin 6))
      (node (ref J1) (pin 8))
      (node (ref J1) (pin 4))
      (node (ref J1) (pin 2))
      (node (ref J1) (pin 10))
      (node (ref J7) (pin 5))
      (node (ref P3) (pin 9))
      (node (ref P3) (pin 6))
      (node (ref P3) (pin 39))
      (node (ref P3) (pin 14))
      (node (ref P3) (pin 34))
      (node (ref P3) (pin 30))
      (node (ref P3) (pin 25))
      (node (ref P3) (pin 20))
      (node (ref J6) (pin 3))
      (node (ref J9) (pin 5))
      (node (ref J8) (pin 5))
      (node (ref J14) (pin 1))
      (node (ref J16) (pin 1))
      (node (ref J10) (pin 5))
      (node (ref J11) (pin 5)))
    (net (code 4) (name SCL_1)
      (node (ref J8) (pin 4))
      (node (ref P3) (pin 5))
      (node (ref J10) (pin 4))
      (node (ref J7) (pin 4))
      (node (ref J9) (pin 4)))
    (net (code 5) (name SDA_1)
      (node (ref J10) (pin 3))
      (node (ref J7) (pin 3))
      (node (ref P3) (pin 3))
      (node (ref J8) (pin 3))
      (node (ref J9) (pin 3)))
    (net (code 6) (name Y+Out)
      (node (ref D2) (pin 2))
      (node (ref J8) (pin 2)))
    (net (code 7) (name Z+Out)
      (node (ref J9) (pin 2))
      (node (ref D3) (pin 2)))
    (net (code 8) (name Z+In)
      (node (ref J9) (pin 1))
      (node (ref J1) (pin 5)))
    (net (code 9) (name VbattOut)
      (node (ref J10) (pin 2))
      (node (ref J2) (pin 2)))
    (net (code 10) (name VbattIn)
      (node (ref J2) (pin 1))
      (node (ref J10) (pin 1)))
    (net (code 11) (name +5V)
      (node (ref J6) (pin 1))
      (node (ref P3) (pin 2))
      (node (ref P3) (pin 4)))
    (net (code 12) (name SCL_3)
      (node (ref J12) (pin 4))
      (node (ref J6) (pin 5))
      (node (ref P3) (pin 28))
      (node (ref R1) (pin 2))
      (node (ref J11) (pin 4)))
    (net (code 13) (name SDA_3)
      (node (ref J6) (pin 4))
      (node (ref P3) (pin 27))
      (node (ref J12) (pin 3))
      (node (ref R2) (pin 2))
      (node (ref J11) (pin 3)))
    (net (code 14) (name Y-Out)
      (node (ref J12) (pin 2))
      (node (ref D5) (pin 2)))
    (net (code 15) (name "Net-(J15-Pad1)")
      (node (ref J5) (pin 3))
      (node (ref J15) (pin 1)))
    (net (code 16) (name "Net-(J4-Pad1)")
      (node (ref J4) (pin 1))
      (node (ref J5) (pin 4)))
    (net (code 17) (name "Net-(J3-Pad1)")
      (node (ref J3) (pin 1))
      (node (ref J5) (pin 5)))
    (net (code 18) (name "Net-(J13-Pad1)")
      (node (ref J13) (pin 1))
      (node (ref J5) (pin 2)))
    (net (code 20) (name "Net-(D1-Pad1)")
      (node (ref D1) (pin 1))
      (node (ref D5) (pin 1))
      (node (ref D3) (pin 1))
      (node (ref D2) (pin 1))
      (node (ref J5) (pin 1))
      (node (ref D4) (pin 1)))
    (net (code 21) (name X-Out)
      (node (ref D4) (pin 2))
      (node (ref J11) (pin 2)))
    (net (code 22) (name X-In)
      (node (ref J1) (pin 7))
      (node (ref J11) (pin 1)))
    (net (code 23) (name Y-In)
      (node (ref J1) (pin 9))
      (node (ref J12) (pin 1)))
    (net (code 24) (name X+Out)
      (node (ref D1) (pin 2))
      (node (ref J7) (pin 2)))
    (net (code 25) (name X+In)
      (node (ref J1) (pin 1))
      (node (ref J7) (pin 1)))
    (net (code 26) (name "Net-(P3-Pad26)")
      (node (ref P3) (pin 26)))
    (net (code 27) (name "Net-(P3-Pad35)")
      (node (ref P3) (pin 35)))
    (net (code 28) (name "Net-(P3-Pad33)")
      (node (ref P3) (pin 33)))
    (net (code 29) (name "Net-(P3-Pad32)")
      (node (ref P3) (pin 32)))
    (net (code 30) (name "Net-(P3-Pad31)")
      (node (ref P3) (pin 31)))
    (net (code 31) (name "Net-(P3-Pad29)")
      (node (ref P3) (pin 29)))
    (net (code 32) (name "Net-(P3-Pad36)")
      (node (ref P3) (pin 36)))
    (net (code 33) (name "Net-(P3-Pad24)")
      (node (ref P3) (pin 24)))
    (net (code 34) (name "Net-(P3-Pad23)")
      (node (ref P3) (pin 23)))
    (net (code 35) (name "Net-(P3-Pad22)")
      (node (ref P3) (pin 22)))
    (net (code 36) (name "Net-(P3-Pad21)")
      (node (ref P3) (pin 21)))
    (net (code 37) (name "Net-(P3-Pad19)")
      (node (ref P3) (pin 19)))
    (net (code 38) (name "Net-(P3-Pad18)")
      (node (ref P3) (pin 18)))
    (net (code 39) (name "Net-(P3-Pad17)")
      (node (ref P3) (pin 17)))
    (net (code 40) (name "Net-(P3-Pad16)")
      (node (ref P3) (pin 16)))
    (net (code 41) (name "Net-(P3-Pad8)")
      (node (ref P3) (pin 8)))
    (net (code 42) (name "Net-(P3-Pad7)")
      (node (ref P3) (pin 7)))
    (net (code 43) (name "Net-(P3-Pad40)")
      (node (ref P3) (pin 40)))
    (net (code 44) (name "Net-(P3-Pad37)")
      (node (ref P3) (pin 37)))
    (net (code 45) (name "Net-(P3-Pad37)")
      (node (ref P3) (pin 37)))
    (net (code 46) (name "Net-(P3-Pad15)")
      (node (ref P3) (pin 15)))
    (net (code 47) (name "Net-(P3-Pad13)")
      (node (ref P3) (pin 13)))
    (net (code 48) (name "Net-(P3-Pad12)")
      (node (ref P3) (pin 12)))
    (net (code 49) (name "Net-(P3-Pad11)")
      (node (ref P3) (pin 11)))
    (net (code 50) (name "Net-(P3-Pad10)")
      (node (ref P3) (pin 10)))))