(export (version D)
  (design
    (source /opt/MMDVM_HS_Dual_Hat/mmdvm_hs_dual_hat.sch)
    (date "Wed 28 Feb 2018 02:36:30 PM CET")
    (tool "Eeschema 5.0.0-rc2-dev-unknown-31e78d6~62~ubuntu17.10.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title MMDVM_HS_Dual_Hat)
        (company DB9MAT+DF2ET+DO7EN)
        (rev 1.0)
        (date 2018-02-05)
        (source mmdvm_hs_dual_hat.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /Power/) (tstamps /5A778C4F/)
      (title_block
        (title MMDVM_HS_Dual_Hat)
        (company DB9MAT+DF2ET+DO7EN)
        (rev 0.1)
        (date 2018-02-05)
        (source Power.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /STM32F103/) (tstamps /5A86EF1A/)
      (title_block
        (title MMDVM_HS_Dual_Hat)
        (company DB9MAT+DF2ET+DO7EN)
        (rev 0.1)
        (date 2018-02-05)
        (source STM32F103.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref R13)
      (value 1k)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/427/rcse3-1013761.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) RCS04021K00JNED)
        (field (name SPR) Mouser)
        (field (name SPN) 71-RCS04021K00JNED))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 589685C3))
    (comp (ref R14)
      (value 1k)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/427/rcse3-1013761.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) RCS04021K00JNED)
        (field (name SPR) Mouser)
        (field (name SPN) 71-RCS04021K00JNED))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58968631))
    (comp (ref C36)
      (value 100n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402V104ZXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402V104ZXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58969AA4))
    (comp (ref C39)
      (value 10n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402Y103KXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402Y103KXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58969E8F))
    (comp (ref C20)
      (value 100n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402V104ZXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402V104ZXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5896DEF7))
    (comp (ref R4)
      (value 3k8)
      (footprint Resistors_SMD:R_0402)
      (datasheet http://www.mouser.com/ds/2/392/susumu_RR_Data_Sheet-358748.pdf)
      (fields
        (field (name MFR) Susumu)
        (field (name MPN) RR0510P-3831-D)
        (field (name SPR) Mouser)
        (field (name SPN) 754-RR0510P-3831D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5896E5F8))
    (comp (ref C16)
      (value 10n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402Y103KXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402Y103KXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5896E97E))
    (comp (ref R2)
      (value 1k1)
      (footprint Resistors_SMD:R_0402)
      (datasheet http://www.mouser.com/ds/2/392/susumu_RR_Data_Sheet-358748.pdf)
      (fields
        (field (name MFR) Susumu)
        (field (name MPN) RR0510P-112-D)
        (field (name SPR) Mouser)
        (field (name SPN) 754-RR0510P-112D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5896F75D))
    (comp (ref U1)
      (value ADF7021)
      (footprint Housings_DFN_QFN:QFN-48-1EP_7x7mm_Pitch0.5mm)
      (datasheet http://www.mouser.com/ds/2/609/ADF7021-878461.pdf)
      (fields
        (field (name MFR) "Analog Devices")
        (field (name MPN) ADF7021BCPZ)
        (field (name SPR) Mouser)
        (field (name SPN) 584-ADF7021BCPZ))
      (libsource (lib adf7021) (part ADF7021))
      (sheetpath (names /) (tstamps /))
      (tstamp 5896FF14))
    (comp (ref C12)
      (value 6p8)
      (footprint Capacitors_SMD:C_0402)
      (datasheet http://www.mouser.com/ds/2/281/c02e-2905.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GJM1555C1H6R8BB01D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GJM1555C1H6R8BB1D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 589705E1))
    (comp (ref L6)
      (value 27n)
      (footprint Inductors_SMD:L_0402)
      (datasheet http://www.mouser.com/ds/2/281/murata_inductors-1186262.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) LQW15AN27NG80D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-LQW15AN27NG80D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part L-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 589706C7))
    (comp (ref C10)
      (value 4p7)
      (footprint Capacitors_SMD:C_0402)
      (datasheet http://www.mouser.com/ds/2/281/c02e-2905.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GRM1555C1H4R7CA01D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GRM1555C1H4R7CA1D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58971A8F))
    (comp (ref C9)
      (value 10p)
      (footprint Capacitors_SMD:C_0402)
      (datasheet http://www.mouser.com/ds/2/281/c02e-2905.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GRM1555C1E100GA01D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GRM1555C1E100GA1D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58971E4D))
    (comp (ref C2)
      (value 6p8)
      (footprint Capacitors_SMD:C_0402)
      (datasheet http://www.mouser.com/ds/2/281/c02e-2905.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GJM1555C1H6R8BB01D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GJM1555C1H6R8BB1D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58972AD9))
    (comp (ref L2)
      (value 22n)
      (footprint Inductors_SMD:L_0402)
      (datasheet http://www.mouser.com/ds/2/281/JELF243A-0140-937123.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) LQW15CA22NJ00D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-LQW15CA22NJ00D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part L-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58972EEA))
    (comp (ref L8)
      (value 13n)
      (footprint Inductors_SMD:L_0402)
      (datasheet http://www.mouser.com/ds/2/281/murata_inductors-1186262.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) LQW15AN13NG80D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-LQW15AN13NG80D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part L-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58973BF8))
    (comp (ref C8)
      (value 220p)
      (footprint Capacitors_SMD:C_0402)
      (datasheet http://www.mouser.com/ds/2/281/c02e-2905.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GRM1555C1H221JA01D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GRM1555C1H221JA01))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58973FC2))
    (comp (ref C18)
      (value 10n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402Y103KXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402Y103KXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58974124))
    (comp (ref C24)
      (value 22n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet http://www.mouser.com/ds/2/281/c03e-806517.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GCM155R71E223KA55D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GCM155R71E223KA5D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 589757AF))
    (comp (ref R6)
      (value 3r9)
      (footprint Resistors_SMD:R_0402)
      (datasheet http://www.mouser.com/ds/2/427/dcrcwe3-109170.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) CRCW04023R90JNED)
        (field (name SPR) Mouser)
        (field (name SPN) 71-CRCW0402J-3.9-E3))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58976039))
    (comp (ref C14)
      (value 100n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402V104ZXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402V104ZXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 589762ED))
    (comp (ref C4)
      (value 10n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402Y103KXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402Y103KXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 589765ED))
    (comp (ref R8)
      (value 560)
      (footprint Resistors_SMD:R_0402)
      (datasheet http://www.mouser.com/ds/2/315/AOA0000C237-1100991.pdf)
      (fields
        (field (name MFR) Panasonic)
        (field (name MPN) ERA-2AEB561X)
        (field (name SPR) Mouser)
        (field (name SPN) 667-ERA-2AEB561X))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58977A3D))
    (comp (ref R10)
      (value 270)
      (footprint Resistors_SMD:R_0402)
      (datasheet http://www.mouser.com/ds/2/315/AOA0000C237-1100991.pdf)
      (fields
        (field (name MFR) Panasonic)
        (field (name MPN) ERA-2AEB271X)
        (field (name SPR) Mouser)
        (field (name SPN) 667-ERA-2AEB271X))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58977B33))
    (comp (ref C22)
      (value 470p)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/281/c03e-516224.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GCG1555G1H471JA01D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GCG1555G1H471JA1D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58977C18))
    (comp (ref C26)
      (value 15n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/281/c02e-2905.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GRM155R71C153KA01J)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GRM155R71C153KA1J))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58977D12))
    (comp (ref C28)
      (value 1n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet http://www.mouser.com/ds/2/281/c02e-2905.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GRM155R60J102KA01D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GRM155R60J102KA1D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58977DF7))
    (comp (ref C32)
      (value 10n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402Y103KXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402Y103KXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58979714))
    (comp (ref C30)
      (value 100n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402V104ZXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402V104ZXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58979B33))
    (comp (ref X1)
      (value TCXO)
      (footprint Crystals:Crystal_SMD_3225-4pin_3.2x2.5mm)
      (datasheet http://www.mouser.com/ds/2/122/ECS-TXO-3225-608196.pdf)
      (fields
        (field (name MFR) ECS)
        (field (name MPN) ECS-TXO-3225-147.4-TR)
        (field (name SPR) Mouser)
        (field (name SPN) 520-TXO-3225-14.74T))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part TCXO_DFAS11-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5897A831))
    (comp (ref C42)
      (value 10n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402Y103KXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402Y103KXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5897B23C))
    (comp (ref C34)
      (value 22p)
      (footprint Capacitors_SMD:C_0402)
      (datasheet http://www.mouser.com/ds/2/40/C0GNP0-Dielectric-951274.pdf)
      (fields
        (field (name MFR) AVX)
        (field (name MPN) 04025A220GAT2A)
        (field (name SPR) Mouser)
        (field (name SPN) 581-04025A220G))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5897BA0E))
    (comp (ref P2)
      (value SMA)
      (footprint Connectors:SMA_THT_Jack_Straight)
      (datasheet http://www.mouser.com/ds/2/18/C901-144-8RFX-710432.pdf)
      (fields
        (field (name MFR) "TE Connectivity")
        (field (name MPN) 5-1814832-1)
        (field (name SPR) Mouser)
        (field (name SPN) 571-5-1814832-1))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part CONN_01X02-conn-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5897CEF8))
    (comp (ref L4)
      (value 20n)
      (footprint Inductors_SMD:L_0402)
      (datasheet http://www.mouser.com/ds/2/418/NG_CD_1624112_BA1-656883.pdf)
      (fields
        (field (name MFR) "TE Connectivity / Sigma Inductors")
        (field (name MPN) 36501E20NJTDG)
        (field (name SPR) Mouser)
        (field (name SPN) 279-36501E20NJTDG))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part L-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 58972852))
    (comp (ref R11)
      (value 1k)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/427/rcse3-1013761.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) RCS04021K00JNED)
        (field (name SPR) Mouser)
        (field (name SPN) 71-RCS04021K00JNED))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A726))
    (comp (ref R12)
      (value 1k)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/427/rcse3-1013761.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) RCS04021K00JNED)
        (field (name SPR) Mouser)
        (field (name SPN) 71-RCS04021K00JNED))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A731))
    (comp (ref C35)
      (value 100n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402V104ZXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402V104ZXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A748))
    (comp (ref C38)
      (value 10n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402Y103KXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402Y103KXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A753))
    (comp (ref C19)
      (value 100n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402V104ZXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402V104ZXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A776))
    (comp (ref R3)
      (value 3k8)
      (footprint Resistors_SMD:R_0402)
      (datasheet http://www.mouser.com/ds/2/392/susumu_RR_Data_Sheet-358748.pdf)
      (fields
        (field (name MFR) Susumu)
        (field (name MPN) RR0510P-3831-D)
        (field (name SPR) Mouser)
        (field (name SPN) 754-RR0510P-3831D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A787))
    (comp (ref C15)
      (value 10n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402Y103KXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402Y103KXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A798))
    (comp (ref R1)
      (value 1k1)
      (footprint Resistors_SMD:R_0402)
      (datasheet http://www.mouser.com/ds/2/392/susumu_RR_Data_Sheet-358748.pdf)
      (fields
        (field (name MFR) Susumu)
        (field (name MPN) RR0510P-112-D)
        (field (name SPR) Mouser)
        (field (name SPN) 754-RR0510P-112D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A7A9))
    (comp (ref U2)
      (value ADF7021)
      (footprint Housings_DFN_QFN:QFN-48-1EP_7x7mm_Pitch0.5mm)
      (datasheet http://www.mouser.com/ds/2/609/ADF7021-878461.pdf)
      (fields
        (field (name MFR) "Analog Devices")
        (field (name MPN) ADF7021BCPZ)
        (field (name SPR) Mouser)
        (field (name SPN) 584-ADF7021BCPZ))
      (libsource (lib adf7021) (part ADF7021))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A7BA))
    (comp (ref C11)
      (value 6p8)
      (footprint Capacitors_SMD:C_0402)
      (datasheet http://www.mouser.com/ds/2/281/c02e-2905.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GJM1555C1H6R8BB01D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GJM1555C1H6R8BB1D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A7C5))
    (comp (ref L5)
      (value 27n)
      (footprint Inductors_SMD:L_0402)
      (datasheet http://www.mouser.com/ds/2/281/murata_inductors-1186262.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) LQW15AN27NG80D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-LQW15AN27NG80D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part L-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A7D0))
    (comp (ref C7)
      (value 4p7)
      (footprint Capacitors_SMD:C_0402)
      (datasheet http://www.mouser.com/ds/2/281/c02e-2905.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GRM1555C1H4R7CA01D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GRM1555C1H4R7CA1D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A7E7))
    (comp (ref C6)
      (value 10p)
      (footprint Capacitors_SMD:C_0402)
      (datasheet http://www.mouser.com/ds/2/281/c02e-2905.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GRM1555C1E100GA01D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GRM1555C1E100GA1D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A7F2))
    (comp (ref C1)
      (value 6p8)
      (footprint Capacitors_SMD:C_0402)
      (datasheet http://www.mouser.com/ds/2/281/c02e-2905.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GJM1555C1H6R8BB01D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GJM1555C1H6R8BB1D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A7FD))
    (comp (ref L1)
      (value 22n)
      (footprint Inductors_SMD:L_0402)
      (datasheet http://www.mouser.com/ds/2/281/JELF243A-0140-937123.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) LQW15CA22NJ00D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-LQW15CA22NJ00D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part L-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A80E))
    (comp (ref L7)
      (value 13n)
      (footprint Inductors_SMD:L_0402)
      (datasheet http://www.mouser.com/ds/2/281/murata_inductors-1186262.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) LQW15AN13NG80D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-LQW15AN13NG80D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part L-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A819))
    (comp (ref C5)
      (value 220p)
      (footprint Capacitors_SMD:C_0402)
      (datasheet http://www.mouser.com/ds/2/281/c02e-2905.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GRM1555C1H221JA01D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GRM1555C1H221JA01))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A824))
    (comp (ref C17)
      (value 10n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402Y103KXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402Y103KXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A82F))
    (comp (ref C23)
      (value 22n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet http://www.mouser.com/ds/2/281/c03e-806517.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GCM155R71E223KA55D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GCM155R71E223KA5D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A84C))
    (comp (ref R5)
      (value 3r9)
      (footprint Resistors_SMD:R_0402)
      (datasheet http://www.mouser.com/ds/2/427/dcrcwe3-109170.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) CRCW04023R90JNED)
        (field (name SPR) Mouser)
        (field (name SPN) 71-CRCW0402J-3.9-E3))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A857))
    (comp (ref C13)
      (value 100n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402V104ZXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402V104ZXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A862))
    (comp (ref C3)
      (value 10n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402Y103KXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402Y103KXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A86D))
    (comp (ref R7)
      (value 560)
      (footprint Resistors_SMD:R_0402)
      (datasheet http://www.mouser.com/ds/2/315/AOA0000C237-1100991.pdf)
      (fields
        (field (name MFR) Panasonic)
        (field (name MPN) ERA-2AEB561X)
        (field (name SPR) Mouser)
        (field (name SPN) 667-ERA-2AEB561X))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A884))
    (comp (ref R9)
      (value 270)
      (footprint Resistors_SMD:R_0402)
      (datasheet http://www.mouser.com/ds/2/315/AOA0000C237-1100991.pdf)
      (fields
        (field (name MFR) Panasonic)
        (field (name MPN) ERA-2AEB271X)
        (field (name SPR) Mouser)
        (field (name SPN) 667-ERA-2AEB271X))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A88F))
    (comp (ref C21)
      (value 470p)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/281/c03e-516224.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GCG1555G1H471JA01D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GCG1555G1H471JA1D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A89A))
    (comp (ref C25)
      (value 15n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/281/c02e-2905.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GRM155R71C153KA01J)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GRM155R71C153KA1J))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A8A5))
    (comp (ref C27)
      (value 1n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet http://www.mouser.com/ds/2/281/c02e-2905.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GRM155R60J102KA01D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GRM155R60J102KA1D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A8B0))
    (comp (ref C31)
      (value 10n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402Y103KXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402Y103KXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A8BB))
    (comp (ref C29)
      (value 100n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402V104ZXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402V104ZXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A8CC))
    (comp (ref C33)
      (value 22p)
      (footprint Capacitors_SMD:C_0402)
      (datasheet http://www.mouser.com/ds/2/40/C0GNP0-Dielectric-951274.pdf)
      (fields
        (field (name MFR) AVX)
        (field (name MPN) 04025A220GAT2A)
        (field (name SPR) Mouser)
        (field (name SPN) 581-04025A220G))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A8FF))
    (comp (ref L3)
      (value 20n)
      (footprint Inductors_SMD:L_0402)
      (datasheet http://www.mouser.com/ds/2/418/NG_CD_1624112_BA1-656883.pdf)
      (fields
        (field (name MFR) "TE Connectivity / Sigma Inductors")
        (field (name MPN) 36501E20NJTDG)
        (field (name SPR) Mouser)
        (field (name SPN) 279-36501E20NJTDG))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part L-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68A946))
    (comp (ref P1)
      (value SMA)
      (footprint Connectors:SMA_THT_Jack_Straight)
      (datasheet http://www.mouser.com/ds/2/18/C901-144-8RFX-710432.pdf)
      (fields
        (field (name MFR) "TE Connectivity")
        (field (name MPN) 5-1814832-1)
        (field (name SPR) Mouser)
        (field (name SPN) 571-5-1814832-1))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part CONN_01X02-conn-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A68D98C))
    (comp (ref R15)
      (value 10k)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/427/crcwce3-1223726.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) CRCW040210K0JNEDC)
        (field (name SPR) Mouser)
        (field (name SPN) 71-CRCW040210K0JNEDC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A7E28BE))
    (comp (ref C43)
      (value 100n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402V104ZXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402V104ZXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A7E28CA))
    (comp (ref SW1)
      (value DNI)
      (footprint Buttons_Switches_SMD:SW_SPST_B3U-1000P)
      (datasheet http://www.mouser.com/ds/2/307/en-b3u-3615.pdf)
      (fields
        (field (name MFR) "Omron Electronics")
        (field (name MPN) B3U-1000P)
        (field (name SPR) Mouser)
        (field (name SPN) 653-B3U-1000P))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part SW_DIP_x01-RESCUE-mmdvm_hs-hat-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A7E28DC))
    (comp (ref C44)
      (value 100n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402V104ZXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402V104ZXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A7E323F))
    (comp (ref C45)
      (value 100n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402V104ZXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402V104ZXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A7E324B))
    (comp (ref C46)
      (value 100n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402V104ZXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402V104ZXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A7E3257))
    (comp (ref R25)
      (value 10k)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/427/crcwce3-1223726.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) CRCW040210K0JNEDC)
        (field (name SPR) Mouser)
        (field (name SPN) 71-CRCW040210K0JNEDC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A842562))
    (comp (ref D1)
      (value green)
      (footprint LEDs:LED_0402)
      (datasheet http://www.mouser.com/ds/2/216/APHHS1005CGCK-38896.pdf)
      (fields
        (field (name MFR) Kingbright)
        (field (name MPN) APHHS1005CGCK)
        (field (name SPR) Mouser)
        (field (name SPN) 604-APHHS1005CGCK))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part LED-RESCUE-mmdvm_hs-hat-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A84256D))
    (comp (ref D2)
      (value yellow)
      (footprint LEDs:LED_0402)
      (datasheet https://www.mouser.com/ds/2/216/APHHS1005SYCK-76875.pdf)
      (fields
        (field (name MFR) Kingbright)
        (field (name MPN) APHHS1005SYCK)
        (field (name SPR) Mouser)
        (field (name SPN) 604-APHHS1005SYCK))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part LED-RESCUE-mmdvm_hs-hat-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A842578))
    (comp (ref D3)
      (value red)
      (footprint LEDs:LED_0402)
      (datasheet http://www.mouser.com/ds/2/216/APHHS1005SURCK-32322.pdf)
      (fields
        (field (name MFR) Kingbright)
        (field (name MPN) APHHS1005SURCK)
        (field (name SPR) Mouser)
        (field (name SPN) 604-APHHS1005SURCK))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part LED-RESCUE-mmdvm_hs-hat-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A842583))
    (comp (ref D4)
      (value yellow)
      (footprint LEDs:LED_0402)
      (datasheet https://www.mouser.com/ds/2/216/APHHS1005SYCK-76875.pdf)
      (fields
        (field (name MFR) Kingbright)
        (field (name MPN) APHHS1005SYCK)
        (field (name SPR) Mouser)
        (field (name SPN) 604-APHHS1005SYCK))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part LED-RESCUE-mmdvm_hs-hat-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A84258E))
    (comp (ref D5)
      (value green)
      (footprint LEDs:LED_0402)
      (datasheet http://www.mouser.com/ds/2/216/APHHS1005CGCK-38896.pdf)
      (fields
        (field (name MFR) Kingbright)
        (field (name MPN) APHHS1005CGCK)
        (field (name SPR) Mouser)
        (field (name SPN) 604-APHHS1005CGCK))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part LED-RESCUE-mmdvm_hs-hat-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A842599))
    (comp (ref D6)
      (value amber)
      (footprint LEDs:LED_0402)
      (datasheet https://www.mouser.com/ds/2/216/APHHS1005SECK-36485.pdf)
      (fields
        (field (name MFR) Kingbright)
        (field (name MPN) APHHS1005SECK)
        (field (name SPR) Mouser)
        (field (name SPN) 604-APHHS1005SECK))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part LED-RESCUE-mmdvm_hs-hat-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8425A4))
    (comp (ref D7)
      (value red)
      (footprint LEDs:LED_0402)
      (datasheet http://www.mouser.com/ds/2/216/APHHS1005SURCK-32322.pdf)
      (fields
        (field (name MFR) Kingbright)
        (field (name MPN) APHHS1005SURCK)
        (field (name SPR) Mouser)
        (field (name SPN) 604-APHHS1005SURCK))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part LED-RESCUE-mmdvm_hs-hat-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8425AF))
    (comp (ref R16)
      (value 1k)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/427/rcse3-1013761.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) RCS04021K00JNED)
        (field (name SPR) Mouser)
        (field (name SPN) 71-RCS04021K00JNED))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8425BB))
    (comp (ref R17)
      (value 1k)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/427/rcse3-1013761.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) RCS04021K00JNED)
        (field (name SPR) Mouser)
        (field (name SPN) 71-RCS04021K00JNED))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8425C7))
    (comp (ref R18)
      (value 1k)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/427/rcse3-1013761.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) RCS04021K00JNED)
        (field (name SPR) Mouser)
        (field (name SPN) 71-RCS04021K00JNED))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8425D3))
    (comp (ref R19)
      (value 1k)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/427/rcse3-1013761.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) RCS04021K00JNED)
        (field (name SPR) Mouser)
        (field (name SPN) 71-RCS04021K00JNED))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8425DF))
    (comp (ref R20)
      (value 1k)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/427/rcse3-1013761.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) RCS04021K00JNED)
        (field (name SPR) Mouser)
        (field (name SPN) 71-RCS04021K00JNED))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8425EB))
    (comp (ref R21)
      (value 1k)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/427/rcse3-1013761.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) RCS04021K00JNED)
        (field (name SPR) Mouser)
        (field (name SPN) 71-RCS04021K00JNED))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8425F7))
    (comp (ref R22)
      (value 1k)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/427/rcse3-1013761.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) RCS04021K00JNED)
        (field (name SPR) Mouser)
        (field (name SPN) 71-RCS04021K00JNED))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A842602))
    (comp (ref D0)
      (value red)
      (footprint LEDs:LED_0402)
      (datasheet http://www.mouser.com/ds/2/216/APHHS1005SURCK-32322.pdf)
      (fields
        (field (name MFR) Kingbright)
        (field (name MPN) APHHS1005SURCK)
        (field (name SPR) Mouser)
        (field (name SPN) 604-APHHS1005SURCK))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part LED-RESCUE-mmdvm_hs-hat-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A842643))
    (comp (ref R24)
      (value 1k)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/427/rcse3-1013761.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) RCS04021K00JNED)
        (field (name SPR) Mouser)
        (field (name SPN) 71-RCS04021K00JNED))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A84264F))
    (comp (ref J1)
      (value RPi_GPIO)
      (footprint Pin_Headers:Pin_Header_Straight_2x20)
      (datasheet https://www.mouser.com/ds/2/181/M20-783-1133465.pdf)
      (fields
        (field (name MFR) Harwin)
        (field (name MPN) M20-7832046)
        (field (name SPR) Mouser)
        (field (name SPN) 855-M20-7832046))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part RPi_GPIO-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8426B4))
    (comp (ref D8)
      (value blue)
      (footprint LEDs:LED_0402)
      (datasheet https://www.mouser.com/ds/2/216/APHHS1005QBC-D-54846.pdf)
      (fields
        (field (name MFR) Kingbright)
        (field (name MPN) " APHHS1005QBC/D")
        (field (name SPR) Mouser)
        (field (name SPN) 604-APHHS1005QBCD))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part LED-RESCUE-mmdvm_hs-hat-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8426D3))
    (comp (ref R23)
      (value 1k)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/427/rcse3-1013761.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) RCS04021K00JNED)
        (field (name SPR) Mouser)
        (field (name SPN) 71-RCS04021K00JNED))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8426DF))
    (comp (ref P7)
      (value CONN_02X03)
      (footprint Pin_Headers:Pin_Header_Straight_2x03)
      (datasheet https://www.mouser.com/ds/2/418/NG_CD_826629_AA_baseFilename-774094.pdf)
      (fields
        (field (name MFR) "TE Connectivity / AMP")
        (field (name MPN) " 826632-3")
        (field (name SPR) Mouser)
        (field (name SPN) 571-826632-3))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part CONN_02X03-conn-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8AD6E0))
    (comp (ref R28)
      (value 1k5)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/315/AOA0000C307-1149632.pdf)
      (fields
        (field (name MFR) Panasonic)
        (field (name MPN) ERA-2AED152X)
        (field (name SPR) Mouser)
        (field (name SPN) 667-ERA-2AED152X))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8AD6F0))
    (comp (ref L9)
      (value 100MHz)
      (footprint Inductors_SMD:L_0402)
      (datasheet http://www.mouser.com/ds/2/445/74279277-372706.pdf)
      (fields
        (field (name MFR) "Wurth Electronics")
        (field (name MPN) 74279277)
        (field (name SPR) Mouser)
        (field (name SPN) 710-74279277))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part L-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8AD704))
    (comp (ref C49)
      (value 10n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402Y103KXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402Y103KXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8AD719))
    (comp (ref C48)
      (value 47p)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/281/c02e-2905.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GRM1555C1H470FA01D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GRM1555C1H470FA1D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8AD730))
    (comp (ref C47)
      (value 47p)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/281/c02e-2905.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GRM1555C1H470FA01D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GRM1555C1H470FA1D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8AD737))
    (comp (ref R27)
      (value 27R)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/392/susumu_RR_Data_Sheet-1206438.pdf)
      (fields
        (field (name MFR) Susumu)
        (field (name MPN) RR0510R-270-D)
        (field (name SPR) Mouser)
        (field (name SPN) 754-RR0510R-270D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8AD73E))
    (comp (ref R26)
      (value 27R)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/392/susumu_RR_Data_Sheet-1206438.pdf)
      (fields
        (field (name MFR) Susumu)
        (field (name MPN) RR0510R-270-D)
        (field (name SPR) Mouser)
        (field (name SPN) 754-RR0510R-270D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8AD745))
    (comp (ref P8)
      (value USB_OTG)
      (footprint MMDVM:USB-mini-710-65100516121)
      (datasheet https://www.mouser.com/ds/2/445/65100516121-537838.pdf)
      (fields
        (field (name MFR) "Wurth Electronics")
        (field (name MPN) 65100516121)
        (field (name SPR) Mouser)
        (field (name SPN) 710-65100516121))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part USB_OTG-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8AD758))
    (comp (ref C50)
      (value 100n)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/427/vjw1bcbascomseries-223529.pdf)
      (fields
        (field (name MFR) "Vishay / Vitramon")
        (field (name MPN) VJ0402V104ZXJCW1BC)
        (field (name SPR) Mouser)
        (field (name SPN) 77-VJ0402V104ZXJCBC))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8EDEA6))
    (comp (ref L10)
      (value 10u)
      (footprint Inductors_SMD:L_0402)
      (datasheet http://www.mouser.com/ds/2/445/74279277-372706.pdf)
      (fields
        (field (name MFR) "Wurth Electronics")
        (field (name MPN) 74279277)
        (field (name SPR) Mouser)
        (field (name SPN) 710-74279277))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part L-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8EDEB2))
    (comp (ref C51)
      (value 10u/10V)
      (footprint Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow)
      (datasheet https://www.mouser.com/ds/2/40/TPS_AUTO-845414.pdf)
      (fields
        (field (name MFR) AVX)
        (field (name MPN) TPSA106K010T0900)
        (field (name SPR) Mouser)
        (field (name SPN) 581-TPSA106K010T0900))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part CP-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8EDECA))
    (comp (ref C52)
      (value 10u)
      (footprint Capacitors_SMD:C_0402)
      (datasheet https://www.mouser.com/ds/2/281/Murata%20GJM%20Series-1186094.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GRM155C80J106ME11J)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GRM155C80J106ME1J))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8EDEDC))
    (comp (ref U4)
      (value LD1117S33TR)
      (footprint TO_SOT_Packages_SMD:SOT-223-3_TabPin2)
      (datasheet https://www.mouser.com/ds/2/268/21665b-63633.pdf)
      (fields
        (field (name SPR) Mouser)
        (field (name MFR) "Microchip Technology")
        (field (name MPN) TC2117-3.3VDBTR)
        (field (name SPN) 579-TC2117-3.3VDBTR))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part LD1117S33TR-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A8EDEF3))
    (comp (ref P4)
      (value DISPLAY)
      (footprint Pin_Headers:Pin_Header_Straight_1x04)
      (datasheet http://www.mouser.com/ds/2/418/NG_CD_826629_AA_baseFilename-683270.pdf)
      (fields
        (field (name MFR) "TE Connectivity / AMP")
        (field (name MPN) 826629-4)
        (field (name SPR) Mouser)
        (field (name SPN) 571-826629-4))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part CONN_01X04-conn-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A7D83E9))
    (comp (ref P3)
      (value I2C)
      (footprint Pin_Headers:Pin_Header_Straight_1x04)
      (datasheet http://www.mouser.com/ds/2/418/NG_CD_826629_AA_baseFilename-683270.pdf)
      (fields
        (field (name MFR) "TE Connectivity / AMP")
        (field (name MPN) 826629-4)
        (field (name SPR) Mouser)
        (field (name SPN) 571-826629-4))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part CONN_01X04-conn-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A7D83FB))
    (comp (ref P5)
      (value STLINK)
      (footprint Pin_Headers:Pin_Header_Straight_1x04)
      (datasheet http://www.mouser.com/ds/2/418/NG_CD_826629_AA_baseFilename-683270.pdf)
      (fields
        (field (name MFR) "TE Connectivity / AMP")
        (field (name MPN) 826629-4)
        (field (name SPR) Mouser)
        (field (name SPN) 571-826629-4))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part CONN_01X04-conn-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A7ED3C6))
    (comp (ref R30)
      (value 100k)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/427/dcrcwe3-109170.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) CRCW0402100KFKED)
        (field (name SPR) Mouser)
        (field (name SPN) 71-CRCW0402-100K-E3))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A89671B))
    (comp (ref R29)
      (value 100k)
      (footprint Resistors_SMD:R_0402)
      (datasheet https://www.mouser.com/ds/2/427/dcrcwe3-109170.pdf)
      (fields
        (field (name MFR) Vishay)
        (field (name MPN) CRCW0402100KFKED)
        (field (name SPR) Mouser)
        (field (name SPN) 71-CRCW0402-100K-E3))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /Power/) (tstamps /5A778C4F/))
      (tstamp 5A896849))
    (comp (ref Y1)
      (value 8MHz)
      (footprint Crystals:Crystal_SMD_Abracon_ABM3-2pin_5.0x3.2mm)
      (datasheet http://www.mouser.com/ds/2/3/abm3-47699.pdf)
      (fields
        (field (name MFR) ABRACON)
        (field (name MPN) ABM3-8.000MHz-D2Y-T)
        (field (name SPR) Mouser)
        (field (name SPN) 815-ABM3-8-D2Y-T))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part Crystal-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /STM32F103/) (tstamps /5A86EF1A/))
      (tstamp 5A775536))
    (comp (ref C40)
      (value 20p)
      (footprint Capacitors_SMD:C_0402)
      (datasheet http://www.mouser.com/ds/2/281/c02e-2905.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GJM1555C1H200FB01D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GJM1555C1H200FB1D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /STM32F103/) (tstamps /5A86EF1A/))
      (tstamp 5A775542))
    (comp (ref C41)
      (value 20p)
      (footprint Capacitors_SMD:C_0402)
      (datasheet http://www.mouser.com/ds/2/281/c02e-2905.pdf)
      (fields
        (field (name MFR) "Murata Electronics")
        (field (name MPN) GJM1555C1H200FB01D)
        (field (name SPR) Mouser)
        (field (name SPN) 81-GJM1555C1H200FB1D))
      (libsource (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue))
      (sheetpath (names /STM32F103/) (tstamps /5A86EF1A/))
      (tstamp 5A77554E))
    (comp (ref U3)
      (value STM32F103C8T6)
      (footprint Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm)
      (datasheet http://www.mouser.com/ds/2/389/stm32f103c8-956229.pdf)
      (fields
        (field (name MFR) STMicroelectronics)
        (field (name MPN) STM32F103C8T6)
        (field (name SPR) Mouser)
        (field (name SPN) 511-STM32F103C8T6))
      (libsource (lib stm32f103c8t6) (part STM32F103C8T6))
      (sheetpath (names /STM32F103/) (tstamps /5A86EF1A/))
      (tstamp 5A775653)))
  (libparts
    (libpart (lib adf7021) (part ADF7021)
      (fields
        (field (name Reference) U)
        (field (name Value) ADF7021))
      (pins
        (pin (num 1) (name VCOIN) (type input))
        (pin (num 2) (name CREG1) (type input))
        (pin (num 3) (name VDD1) (type input))
        (pin (num 4) (name RFOUT) (type input))
        (pin (num 5) (name RFGND) (type input))
        (pin (num 6) (name RFIN) (type input))
        (pin (num 7) (name RFINB) (type input))
        (pin (num 8) (name RLNA) (type input))
        (pin (num 9) (name VDD4) (type input))
        (pin (num 10) (name RSET) (type input))
        (pin (num 11) (name CREG4) (type input))
        (pin (num 12) (name GND4) (type input))
        (pin (num 13) (name MIX_I) (type input))
        (pin (num 14) (name NMIX_I) (type input))
        (pin (num 15) (name MIX_Q) (type input))
        (pin (num 16) (name NMIX_Q) (type input))
        (pin (num 17) (name FILT_I) (type input))
        (pin (num 18) (name NFILT_I) (type input))
        (pin (num 19) (name GND4) (type input))
        (pin (num 20) (name FILT_Q) (type input))
        (pin (num 21) (name NFILT_Q) (type input))
        (pin (num 22) (name GND4) (type input))
        (pin (num 23) (name TEST_A) (type input))
        (pin (num 24) (name CE) (type input))
        (pin (num 25) (name SLE) (type input))
        (pin (num 26) (name SDATA) (type input))
        (pin (num 27) (name SREAD) (type input))
        (pin (num 28) (name SCLK) (type input))
        (pin (num 29) (name GND2) (type input))
        (pin (num 30) (name ADCIN) (type input))
        (pin (num 31) (name CREG2) (type input))
        (pin (num 32) (name VDD2) (type input))
        (pin (num 33) (name SWD) (type input))
        (pin (num 34) (name TxRxDATA) (type input))
        (pin (num 35) (name TxRxCLK) (type input))
        (pin (num 36) (name CLKOUT) (type input))
        (pin (num 37) (name MUXOUT) (type input))
        (pin (num 38) (name OSC2) (type input))
        (pin (num 39) (name OSC1) (type input))
        (pin (num 40) (name VDD3) (type input))
        (pin (num 41) (name CREG3) (type input))
        (pin (num 42) (name CPOUT) (type input))
        (pin (num 43) (name VDD) (type input))
        (pin (num 44) (name L2) (type input))
        (pin (num 45) (name GND) (type input))
        (pin (num 46) (name L1) (type input))
        (pin (num 47) (name GND1) (type input))
        (pin (num 48) (name CVCO) (type input))
        (pin (num 49) (name EPAD) (type input))))
    (libpart (lib mmdvm_hs_dual_hat-rescue) (part C-device-mmdvm_hs_dual_hat-rescue)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C-device-mmdvm_hs_dual_hat-rescue))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib mmdvm_hs_dual_hat-rescue) (part CONN_01X02-conn-mmdvm_hs_dual_hat-rescue)
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02-conn-mmdvm_hs_dual_hat-rescue))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib mmdvm_hs_dual_hat-rescue) (part CONN_01X04-conn-mmdvm_hs_dual_hat-rescue)
      (footprints
        (fp Pin_Header_Straight_1X04)
        (fp Pin_Header_Angled_1X04)
        (fp Socket_Strip_Straight_1X04)
        (fp Socket_Strip_Angled_1X04))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X04-conn-mmdvm_hs_dual_hat-rescue))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib mmdvm_hs_dual_hat-rescue) (part CONN_02X03-conn-mmdvm_hs_dual_hat-rescue)
      (footprints
        (fp Pin_Header_Straight_2X03)
        (fp Pin_Header_Angled_2X03)
        (fp Socket_Strip_Straight_2X03)
        (fp Socket_Strip_Angled_2X03))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_02X03-conn-mmdvm_hs_dual_hat-rescue))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib mmdvm_hs_dual_hat-rescue) (part CP-device-mmdvm_hs_dual_hat-rescue)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP-device-mmdvm_hs_dual_hat-rescue))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib mmdvm_hs_dual_hat-rescue) (part Crystal-device-mmdvm_hs_dual_hat-rescue)
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal-device-mmdvm_hs_dual_hat-rescue))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib mmdvm_hs_dual_hat-rescue) (part L-device-mmdvm_hs_dual_hat-rescue)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L-device-mmdvm_hs_dual_hat-rescue))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib mmdvm_hs_dual_hat-rescue) (part LD1117S33TR-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue)
      (footprints
        (fp SOT223))
      (fields
        (field (name Reference) U)
        (field (name Value) LD1117S33TR-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue)
        (field (name Footprint) SOT-223))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))))
    (libpart (lib mmdvm_hs_dual_hat-rescue) (part LED-RESCUE-mmdvm_hs-hat-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue)
      (footprints
        (fp LED*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED-RESCUE-mmdvm_hs-hat-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib mmdvm_hs_dual_hat-rescue) (part R-device-mmdvm_hs_dual_hat-rescue)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R-device-mmdvm_hs_dual_hat-rescue))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib mmdvm_hs_dual_hat-rescue) (part RPi_GPIO-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue)
      (fields
        (field (name Reference) J)
        (field (name Value) RPi_GPIO-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (pins
        (pin (num 1) (name 3.3V) (type power_in))
        (pin (num 2) (name 5V) (type power_in))
        (pin (num 3) (name BCM2_SDA) (type BiDi))
        (pin (num 4) (name 5V) (type power_in))
        (pin (num 5) (name BCM3_SCL) (type BiDi))
        (pin (num 6) (name GND) (type power_in))
        (pin (num 7) (name BCM4_GPCLK0) (type BiDi))
        (pin (num 8) (name BCM14_TXD) (type BiDi))
        (pin (num 9) (name GND) (type power_in))
        (pin (num 10) (name BCM15_RXD) (type BiDi))
        (pin (num 11) (name BCM17) (type BiDi))
        (pin (num 12) (name BCM18_PCM_C) (type BiDi))
        (pin (num 13) (name BCM27_PCM_D) (type BiDi))
        (pin (num 14) (name GND) (type power_in))
        (pin (num 15) (name BCM22) (type BiDi))
        (pin (num 16) (name BCM23) (type BiDi))
        (pin (num 17) (name 3.3V) (type power_in))
        (pin (num 18) (name BCM24) (type BiDi))
        (pin (num 19) (name BCM10_MOSI) (type BiDi))
        (pin (num 20) (name GND) (type power_in))
        (pin (num 21) (name BCM9_MISO) (type BiDi))
        (pin (num 22) (name BCM25) (type BiDi))
        (pin (num 23) (name BCM11_SCLK) (type BiDi))
        (pin (num 24) (name BCM8_CE0) (type BiDi))
        (pin (num 25) (name GND) (type power_in))
        (pin (num 26) (name BCM7_CE1) (type BiDi))
        (pin (num 27) (name BCM0_ID_SD) (type BiDi))
        (pin (num 28) (name BCM1_ID_SC) (type BiDi))
        (pin (num 29) (name BCM5) (type BiDi))
        (pin (num 30) (name GND) (type power_in))
        (pin (num 31) (name BCM6) (type BiDi))
        (pin (num 32) (name BCM12) (type BiDi))
        (pin (num 33) (name BCM13) (type BiDi))
        (pin (num 34) (name GND) (type power_in))
        (pin (num 35) (name BCM19_MISO) (type BiDi))
        (pin (num 36) (name BCM16) (type BiDi))
        (pin (num 37) (name BCM26) (type BiDi))
        (pin (num 38) (name BCM20_MOSI) (type BiDi))
        (pin (num 39) (name GND) (type power_in))
        (pin (num 40) (name BCM21_SCLK) (type BiDi))))
    (libpart (lib stm32f103c8t6) (part STM32F103C8T6)
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F103C8T6))
      (pins
        (pin (num 1) (name VBAT) (type input))
        (pin (num 2) (name PC13) (type input))
        (pin (num 3) (name PC14/OSC32_IN) (type input))
        (pin (num 4) (name PC15/OSC32_OUT) (type input))
        (pin (num 5) (name OSC_IN) (type input))
        (pin (num 6) (name OSC_OUT) (type input))
        (pin (num 7) (name NRST) (type input))
        (pin (num 8) (name VSSA) (type input))
        (pin (num 9) (name VDDA) (type input))
        (pin (num 10) (name PA0) (type input))
        (pin (num 11) (name PA1) (type input))
        (pin (num 12) (name PA2) (type input))
        (pin (num 13) (name PA3) (type input))
        (pin (num 14) (name PA4) (type input))
        (pin (num 15) (name PA5) (type input))
        (pin (num 16) (name PA6) (type input))
        (pin (num 17) (name PA7) (type input))
        (pin (num 18) (name PB0) (type input))
        (pin (num 19) (name PB1) (type input))
        (pin (num 20) (name PB2) (type input))
        (pin (num 21) (name PB10) (type input))
        (pin (num 22) (name PB11) (type input))
        (pin (num 23) (name VSS_1) (type input))
        (pin (num 24) (name VDD_1) (type input))
        (pin (num 25) (name PB12) (type input))
        (pin (num 26) (name PB13) (type input))
        (pin (num 27) (name PB14) (type input))
        (pin (num 28) (name PB15) (type input))
        (pin (num 29) (name PA8) (type input))
        (pin (num 30) (name PA9) (type input))
        (pin (num 31) (name PA10) (type input))
        (pin (num 32) (name PA11) (type input))
        (pin (num 33) (name PA12) (type input))
        (pin (num 34) (name PA13) (type input))
        (pin (num 35) (name VSS_2) (type input))
        (pin (num 36) (name VDD_2) (type input))
        (pin (num 37) (name PA14) (type input))
        (pin (num 38) (name PA15) (type input))
        (pin (num 39) (name PB3) (type input))
        (pin (num 40) (name PB4) (type input))
        (pin (num 41) (name PB5) (type input))
        (pin (num 42) (name PB6) (type input))
        (pin (num 43) (name PB7) (type input))
        (pin (num 44) (name BOOT0) (type input))
        (pin (num 45) (name PB8) (type input))
        (pin (num 46) (name PB9) (type input))
        (pin (num 47) (name VSS_3) (type input))
        (pin (num 48) (name VDD_3) (type input))))
    (libpart (lib mmdvm_hs_dual_hat-rescue) (part SW_DIP_x01-RESCUE-mmdvm_hs-hat-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue)
      (footprints
        (fp SW?DIP?x1*))
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_DIP_x01-RESCUE-mmdvm_hs-hat-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))))
    (libpart (lib mmdvm_hs_dual_hat-rescue) (part TCXO_DFAS11-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue)
      (fields
        (field (name Reference) X)
        (field (name Value) TCXO_DFAS11-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (pins
        (pin (num 1) (name VContr) (type passive))
        (pin (num 2) (name GND) (type passive))
        (pin (num 3) (name FREQ) (type output))
        (pin (num 4) (name VCC) (type power_in))))
    (libpart (lib mmdvm_hs_dual_hat-rescue) (part USB_OTG-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue)
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) P)
        (field (name Value) USB_OTG-RESCUE-mmdvm_hs_dual_hat-mmdvm_hs_dual_hat-rescue))
      (pins
        (pin (num 1) (name VCC) (type power_out))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name ID) (type power_in))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name shield) (type passive)))))
  (libraries
    (library (logical adf7021)
      (uri /opt/MMDVM_HS_Dual_Hat/adf7021.lib))
    (library (logical mmdvm_hs_dual_hat-rescue)
      (uri /opt/MMDVM_HS_Dual_Hat/mmdvm_hs_dual_hat-rescue.lib))
    (library (logical stm32f103c8t6)
      (uri /opt/MMDVM_HS_Dual_Hat/stm32f103c8t6.lib)))
  (nets
    (net (code 1) (name "Net-(C14-Pad1)")
      (node (ref R6) (pin 2))
      (node (ref C14) (pin 1)))
    (net (code 2) (name "Net-(C34-Pad1)")
      (node (ref U1) (pin 39))
      (node (ref C34) (pin 1)))
    (net (code 3) (name "Net-(C22-Pad1)")
      (node (ref U1) (pin 1))
      (node (ref R8) (pin 2))
      (node (ref C22) (pin 1)))
    (net (code 4) (name "Net-(C28-Pad1)")
      (node (ref R10) (pin 1))
      (node (ref R8) (pin 1))
      (node (ref C28) (pin 1))
      (node (ref U1) (pin 42)))
    (net (code 5) (name "Net-(C6-Pad1)")
      (node (ref C6) (pin 1))
      (node (ref L7) (pin 1))
      (node (ref U2) (pin 4)))
    (net (code 6) (name "Net-(R2-Pad1)")
      (node (ref R2) (pin 1))
      (node (ref U1) (pin 8)))
    (net (code 7) (name "Net-(C20-Pad1)")
      (node (ref U1) (pin 11))
      (node (ref C20) (pin 1)))
    (net (code 8) (name "Net-(R4-Pad1)")
      (node (ref R4) (pin 1))
      (node (ref U1) (pin 10)))
    (net (code 9) (name "Net-(C10-Pad1)")
      (node (ref C10) (pin 1))
      (node (ref L6) (pin 2))
      (node (ref U1) (pin 6)))
    (net (code 10) (name "Net-(C12-Pad1)")
      (node (ref U1) (pin 7))
      (node (ref C12) (pin 1))
      (node (ref L6) (pin 1)))
    (net (code 11) (name "Net-(C24-Pad1)")
      (node (ref C24) (pin 1))
      (node (ref U1) (pin 48)))
    (net (code 12) (name "Net-(C24-Pad2)")
      (node (ref C24) (pin 2))
      (node (ref U1) (pin 2))
      (node (ref R6) (pin 1)))
    (net (code 13) (name "Net-(C7-Pad1)")
      (node (ref L5) (pin 2))
      (node (ref C7) (pin 1))
      (node (ref U2) (pin 6)))
    (net (code 14) (name "Net-(C11-Pad1)")
      (node (ref L5) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref U2) (pin 7)))
    (net (code 15) (name "Net-(C1-Pad1)")
      (node (ref L1) (pin 2))
      (node (ref L3) (pin 1))
      (node (ref C1) (pin 1)))
    (net (code 16) (name "Net-(C29-Pad2)")
      (node (ref U2) (pin 41))
      (node (ref C29) (pin 2)))
    (net (code 17) (name "Net-(R12-Pad2)")
      (node (ref U2) (pin 34))
      (node (ref R12) (pin 2)))
    (net (code 18) (name "Net-(C6-Pad2)")
      (node (ref C7) (pin 2))
      (node (ref L3) (pin 2))
      (node (ref C6) (pin 2)))
    (net (code 19) (name "Net-(R11-Pad2)")
      (node (ref U2) (pin 35))
      (node (ref R11) (pin 2)))
    (net (code 20) (name SCLK)
      (node (ref U3) (pin 41))
      (node (ref U2) (pin 28))
      (node (ref U1) (pin 28)))
    (net (code 21) (name SREAD)
      (node (ref U1) (pin 27))
      (node (ref U2) (pin 27))
      (node (ref U3) (pin 43)))
    (net (code 22) (name SDATA)
      (node (ref U2) (pin 26))
      (node (ref U3) (pin 42))
      (node (ref U1) (pin 26)))
    (net (code 23) (name SLE2)
      (node (ref U2) (pin 25))
      (node (ref U3) (pin 16)))
    (net (code 24) (name "Net-(C35-Pad2)")
      (node (ref U2) (pin 31))
      (node (ref C35) (pin 2)))
    (net (code 25) (name "Net-(C9-Pad1)")
      (node (ref C9) (pin 1))
      (node (ref L8) (pin 1))
      (node (ref U1) (pin 4)))
    (net (code 26) (name DATA1)
      (node (ref U3) (pin 40))
      (node (ref R14) (pin 1)))
    (net (code 27) (name DCLK1)
      (node (ref U3) (pin 39))
      (node (ref R13) (pin 1)))
    (net (code 28) (name CE)
      (node (ref U2) (pin 24))
      (node (ref U3) (pin 3))
      (node (ref U1) (pin 24)))
    (net (code 29) (name DATA2)
      (node (ref U3) (pin 14))
      (node (ref R12) (pin 1)))
    (net (code 30) (name DCLK2)
      (node (ref R11) (pin 1))
      (node (ref U3) (pin 15)))
    (net (code 31) (name SLE1)
      (node (ref U1) (pin 25))
      (node (ref U3) (pin 45)))
    (net (code 32) (name "Net-(C10-Pad2)")
      (node (ref L4) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref C10) (pin 2)))
    (net (code 33) (name "Net-(R13-Pad2)")
      (node (ref U1) (pin 35))
      (node (ref R13) (pin 2)))
    (net (code 34) (name "Net-(C2-Pad1)")
      (node (ref L2) (pin 2))
      (node (ref C2) (pin 1))
      (node (ref L4) (pin 1)))
    (net (code 35) (name "Net-(C30-Pad2)")
      (node (ref C30) (pin 2))
      (node (ref U1) (pin 41)))
    (net (code 36) (name "Net-(C36-Pad2)")
      (node (ref C36) (pin 2))
      (node (ref U1) (pin 31)))
    (net (code 37) (name "Net-(R14-Pad2)")
      (node (ref R14) (pin 2))
      (node (ref U1) (pin 34)))
    (net (code 38) (name "Net-(C23-Pad2)")
      (node (ref U2) (pin 2))
      (node (ref R5) (pin 1))
      (node (ref C23) (pin 2)))
    (net (code 39) (name "Net-(C33-Pad1)")
      (node (ref C33) (pin 1))
      (node (ref C34) (pin 2))
      (node (ref X1) (pin 3)))
    (net (code 40) (name "Net-(U2-Pad46)")
      (node (ref U2) (pin 46)))
    (net (code 41) (name "Net-(U2-Pad23)")
      (node (ref U2) (pin 23)))
    (net (code 42) (name "Net-(U2-Pad21)")
      (node (ref U2) (pin 21)))
    (net (code 43) (name "Net-(U2-Pad20)")
      (node (ref U2) (pin 20)))
    (net (code 44) (name "Net-(U2-Pad18)")
      (node (ref U2) (pin 18)))
    (net (code 45) (name "Net-(U2-Pad17)")
      (node (ref U2) (pin 17)))
    (net (code 46) (name "Net-(U2-Pad16)")
      (node (ref U2) (pin 16)))
    (net (code 47) (name "Net-(U2-Pad15)")
      (node (ref U2) (pin 15)))
    (net (code 48) (name "Net-(U2-Pad14)")
      (node (ref U2) (pin 14)))
    (net (code 49) (name "Net-(U2-Pad13)")
      (node (ref U2) (pin 13)))
    (net (code 50) (name "Net-(U2-Pad30)")
      (node (ref U2) (pin 30)))
    (net (code 51) (name "Net-(U2-Pad44)")
      (node (ref U2) (pin 44)))
    (net (code 52) (name "Net-(U2-Pad38)")
      (node (ref U2) (pin 38)))
    (net (code 53) (name "Net-(U2-Pad37)")
      (node (ref U2) (pin 37)))
    (net (code 54) (name "Net-(U2-Pad33)")
      (node (ref U2) (pin 33)))
    (net (code 55) (name "Net-(U2-Pad36)")
      (node (ref U2) (pin 36)))
    (net (code 56) (name "Net-(U1-Pad36)")
      (node (ref U1) (pin 36)))
    (net (code 57) (name "Net-(U1-Pad16)")
      (node (ref U1) (pin 16)))
    (net (code 58) (name "Net-(U1-Pad30)")
      (node (ref U1) (pin 30)))
    (net (code 59) (name "Net-(U1-Pad23)")
      (node (ref U1) (pin 23)))
    (net (code 60) (name "Net-(U1-Pad21)")
      (node (ref U1) (pin 21)))
    (net (code 61) (name "Net-(U1-Pad20)")
      (node (ref U1) (pin 20)))
    (net (code 62) (name "Net-(U1-Pad18)")
      (node (ref U1) (pin 18)))
    (net (code 63) (name "Net-(U1-Pad17)")
      (node (ref U1) (pin 17)))
    (net (code 64) (name "Net-(U1-Pad15)")
      (node (ref U1) (pin 15)))
    (net (code 65) (name "Net-(U1-Pad14)")
      (node (ref U1) (pin 14)))
    (net (code 66) (name "Net-(U1-Pad13)")
      (node (ref U1) (pin 13)))
    (net (code 67) (name "Net-(U1-Pad46)")
      (node (ref U1) (pin 46)))
    (net (code 68) (name "Net-(U1-Pad44)")
      (node (ref U1) (pin 44)))
    (net (code 69) (name "Net-(U1-Pad38)")
      (node (ref U1) (pin 38)))
    (net (code 70) (name "Net-(U1-Pad37)")
      (node (ref U1) (pin 37)))
    (net (code 71) (name "Net-(U1-Pad33)")
      (node (ref U1) (pin 33)))
    (net (code 72) (name "Net-(X1-Pad1)")
      (node (ref X1) (pin 1)))
    (net (code 73) (name "Net-(C13-Pad1)")
      (node (ref R5) (pin 2))
      (node (ref C13) (pin 1)))
    (net (code 74) (name "Net-(C33-Pad2)")
      (node (ref C33) (pin 2))
      (node (ref U2) (pin 39)))
    (net (code 75) (name "Net-(C21-Pad1)")
      (node (ref U2) (pin 1))
      (node (ref C21) (pin 1))
      (node (ref R7) (pin 2)))
    (net (code 76) (name "Net-(C27-Pad1)")
      (node (ref C27) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref U2) (pin 42))
      (node (ref R7) (pin 1)))
    (net (code 77) (name +3V3)
      (node (ref U1) (pin 43))
      (node (ref C3) (pin 1))
      (node (ref U1) (pin 9))
      (node (ref C39) (pin 2))
      (node (ref U1) (pin 40))
      (node (ref U1) (pin 32))
      (node (ref L7) (pin 2))
      (node (ref C5) (pin 1))
      (node (ref C17) (pin 1))
      (node (ref C31) (pin 1))
      (node (ref U3) (pin 36))
      (node (ref C15) (pin 1))
      (node (ref L10) (pin 2))
      (node (ref P7) (pin 1))
      (node (ref P7) (pin 2))
      (node (ref P5) (pin 4))
      (node (ref C51) (pin 1))
      (node (ref C52) (pin 1))
      (node (ref P3) (pin 1))
      (node (ref R16) (pin 2))
      (node (ref R15) (pin 2))
      (node (ref U3) (pin 24))
      (node (ref U3) (pin 48))
      (node (ref U3) (pin 9))
      (node (ref U3) (pin 1))
      (node (ref U2) (pin 40))
      (node (ref U2) (pin 32))
      (node (ref U2) (pin 9))
      (node (ref U2) (pin 3))
      (node (ref U2) (pin 43))
      (node (ref C44) (pin 1))
      (node (ref C45) (pin 1))
      (node (ref C46) (pin 1))
      (node (ref R24) (pin 1))
      (node (ref C38) (pin 2))
      (node (ref C42) (pin 1))
      (node (ref X1) (pin 4))
      (node (ref C4) (pin 1))
      (node (ref C16) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref C18) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref L8) (pin 2))
      (node (ref C32) (pin 1)))
    (net (code 78) (name "Net-(R3-Pad1)")
      (node (ref R3) (pin 1))
      (node (ref U2) (pin 10)))
    (net (code 79) (name "Net-(C19-Pad1)")
      (node (ref U2) (pin 11))
      (node (ref C19) (pin 1)))
    (net (code 80) (name "Net-(R1-Pad1)")
      (node (ref R1) (pin 1))
      (node (ref U2) (pin 8)))
    (net (code 81) (name "Net-(C23-Pad1)")
      (node (ref C23) (pin 1))
      (node (ref U2) (pin 48)))
    (net (code 82) (name "Net-(L2-Pad1)")
      (node (ref L2) (pin 1))
      (node (ref P1) (pin 1)))
    (net (code 83) (name GND)
      (node (ref C45) (pin 2))
      (node (ref J1) (pin 25))
      (node (ref J1) (pin 30))
      (node (ref J1) (pin 34))
      (node (ref J1) (pin 39))
      (node (ref J1) (pin 6))
      (node (ref J1) (pin 9))
      (node (ref D1) (pin 1))
      (node (ref D2) (pin 1))
      (node (ref D3) (pin 1))
      (node (ref J1) (pin 14))
      (node (ref J1) (pin 20))
      (node (ref C48) (pin 1))
      (node (ref U3) (pin 35))
      (node (ref U3) (pin 23))
      (node (ref U3) (pin 47))
      (node (ref C41) (pin 2))
      (node (ref C40) (pin 2))
      (node (ref U3) (pin 8))
      (node (ref D6) (pin 1))
      (node (ref C52) (pin 2))
      (node (ref U4) (pin 1))
      (node (ref P4) (pin 4))
      (node (ref P3) (pin 2))
      (node (ref D4) (pin 1))
      (node (ref D5) (pin 1))
      (node (ref D7) (pin 1))
      (node (ref C43) (pin 2))
      (node (ref SW1) (pin 2))
      (node (ref C44) (pin 2))
      (node (ref C46) (pin 2))
      (node (ref P8) (pin 5))
      (node (ref P8) (pin 6))
      (node (ref C50) (pin 2))
      (node (ref C49) (pin 1))
      (node (ref P7) (pin 5))
      (node (ref P7) (pin 6))
      (node (ref P5) (pin 2))
      (node (ref D8) (pin 1))
      (node (ref C51) (pin 2))
      (node (ref C21) (pin 2))
      (node (ref C25) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref C27) (pin 2))
      (node (ref U1) (pin 49))
      (node (ref C31) (pin 2))
      (node (ref U1) (pin 29))
      (node (ref C19) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref P1) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref U2) (pin 45))
      (node (ref C18) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref U2) (pin 47))
      (node (ref U2) (pin 5))
      (node (ref U1) (pin 19))
      (node (ref C14) (pin 2))
      (node (ref X1) (pin 2))
      (node (ref C35) (pin 1))
      (node (ref C38) (pin 1))
      (node (ref R4) (pin 2))
      (node (ref U1) (pin 47))
      (node (ref C20) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref C32) (pin 2))
      (node (ref C28) (pin 2))
      (node (ref C26) (pin 2))
      (node (ref C22) (pin 2))
      (node (ref U1) (pin 12))
      (node (ref U1) (pin 22))
      (node (ref C36) (pin 1))
      (node (ref U1) (pin 5))
      (node (ref C39) (pin 1))
      (node (ref R2) (pin 2))
      (node (ref U1) (pin 45))
      (node (ref P2) (pin 2))
      (node (ref U2) (pin 49))
      (node (ref C11) (pin 2))
      (node (ref C42) (pin 2))
      (node (ref U2) (pin 29))
      (node (ref C30) (pin 1))
      (node (ref C29) (pin 1))
      (node (ref C5) (pin 2))
      (node (ref C17) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref U2) (pin 19))
      (node (ref C47) (pin 2))
      (node (ref U2) (pin 22))
      (node (ref U2) (pin 12)))
    (net (code 84) (name "Net-(L1-Pad1)")
      (node (ref P2) (pin 1))
      (node (ref L1) (pin 1)))
    (net (code 85) (name "Net-(C26-Pad1)")
      (node (ref C26) (pin 1))
      (node (ref R10) (pin 2)))
    (net (code 86) (name "Net-(C25-Pad1)")
      (node (ref C25) (pin 1))
      (node (ref R9) (pin 2)))
    (net (code 87) (name "Net-(J1-Pad38)")
      (node (ref R25) (pin 2))
      (node (ref J1) (pin 38)))
    (net (code 88) (name TXD)
      (node (ref U3) (pin 30))
      (node (ref J1) (pin 10)))
    (net (code 89) (name "Net-(D8-Pad2)")
      (node (ref R23) (pin 1))
      (node (ref D8) (pin 2)))
    (net (code 90) (name NXDN_LED)
      (node (ref R23) (pin 2))
      (node (ref U3) (pin 29)))
    (net (code 91) (name "Net-(D1-Pad2)")
      (node (ref R16) (pin 1))
      (node (ref D1) (pin 2)))
    (net (code 92) (name COS_LED)
      (node (ref U3) (pin 28))
      (node (ref R17) (pin 2)))
    (net (code 93) (name "Net-(D3-Pad2)")
      (node (ref R18) (pin 1))
      (node (ref D3) (pin 2)))
    (net (code 94) (name PTT_LED)
      (node (ref U3) (pin 27))
      (node (ref R18) (pin 2)))
    (net (code 95) (name DMR_LED)
      (node (ref U3) (pin 26))
      (node (ref R19) (pin 2)))
    (net (code 96) (name "Net-(D5-Pad2)")
      (node (ref D5) (pin 2))
      (node (ref R20) (pin 1)))
    (net (code 97) (name "Net-(D4-Pad2)")
      (node (ref R19) (pin 1))
      (node (ref D4) (pin 2)))
    (net (code 98) (name DSTAR_LED)
      (node (ref R20) (pin 2))
      (node (ref U3) (pin 25)))
    (net (code 99) (name YSF_LED)
      (node (ref U3) (pin 19))
      (node (ref R21) (pin 2)))
    (net (code 100) (name "Net-(D6-Pad2)")
      (node (ref D6) (pin 2))
      (node (ref R21) (pin 1)))
    (net (code 101) (name +5V)
      (node (ref L9) (pin 1))
      (node (ref J1) (pin 2))
      (node (ref J1) (pin 4))
      (node (ref R28) (pin 1))
      (node (ref U4) (pin 3))
      (node (ref P4) (pin 1)))
    (net (code 102) (name "Net-(C49-Pad2)")
      (node (ref L9) (pin 2))
      (node (ref P8) (pin 1))
      (node (ref C49) (pin 2)))
    (net (code 103) (name "Net-(C48-Pad2)")
      (node (ref R28) (pin 2))
      (node (ref P8) (pin 3))
      (node (ref R27) (pin 1))
      (node (ref C48) (pin 2)))
    (net (code 104) (name "Net-(C47-Pad1)")
      (node (ref P8) (pin 2))
      (node (ref C47) (pin 1))
      (node (ref R26) (pin 1)))
    (net (code 105) (name NRST)
      (node (ref SW1) (pin 1))
      (node (ref J1) (pin 40))
      (node (ref U3) (pin 7))
      (node (ref R15) (pin 1))
      (node (ref C43) (pin 1)))
    (net (code 106) (name RXD)
      (node (ref U3) (pin 31))
      (node (ref J1) (pin 8)))
    (net (code 107) (name SWCLK)
      (node (ref U3) (pin 37))
      (node (ref P5) (pin 3)))
    (net (code 108) (name SWDIO)
      (node (ref P5) (pin 1))
      (node (ref U3) (pin 34)))
    (net (code 109) (name SCL)
      (node (ref P3) (pin 3))
      (node (ref J1) (pin 5)))
    (net (code 110) (name SDA)
      (node (ref P3) (pin 4))
      (node (ref J1) (pin 3)))
    (net (code 111) (name DISP_RXD)
      (node (ref U3) (pin 13))
      (node (ref P4) (pin 3)))
    (net (code 112) (name DISP_TXD)
      (node (ref U3) (pin 12))
      (node (ref P4) (pin 2)))
    (net (code 113) (name D-)
      (node (ref R26) (pin 2))
      (node (ref U3) (pin 32)))
    (net (code 114) (name D+)
      (node (ref U3) (pin 33))
      (node (ref R27) (pin 2)))
    (net (code 115) (name BOOT0)
      (node (ref U3) (pin 44))
      (node (ref R25) (pin 1))
      (node (ref R29) (pin 2)))
    (net (code 116) (name BOOT1)
      (node (ref U3) (pin 20))
      (node (ref R30) (pin 1)))
    (net (code 117) (name "Net-(D7-Pad2)")
      (node (ref D7) (pin 2))
      (node (ref R22) (pin 1)))
    (net (code 118) (name "Net-(D0-Pad2)")
      (node (ref D0) (pin 2))
      (node (ref R24) (pin 2)))
    (net (code 119) (name SERVICE)
      (node (ref U3) (pin 2))
      (node (ref D0) (pin 1)))
    (net (code 120) (name P25_LED)
      (node (ref R22) (pin 2))
      (node (ref U3) (pin 18)))
    (net (code 121) (name "Net-(C50-Pad1)")
      (node (ref L10) (pin 1))
      (node (ref C50) (pin 1))
      (node (ref U4) (pin 2)))
    (net (code 122) (name "Net-(J1-Pad35)")
      (node (ref J1) (pin 35)))
    (net (code 123) (name "Net-(P8-Pad4)")
      (node (ref P8) (pin 4)))
    (net (code 124) (name "Net-(J1-Pad17)")
      (node (ref J1) (pin 17)))
    (net (code 125) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1)))
    (net (code 126) (name "Net-(J1-Pad12)")
      (node (ref J1) (pin 12)))
    (net (code 127) (name "Net-(J1-Pad16)")
      (node (ref J1) (pin 16)))
    (net (code 128) (name "Net-(J1-Pad18)")
      (node (ref J1) (pin 18)))
    (net (code 129) (name "Net-(J1-Pad22)")
      (node (ref J1) (pin 22)))
    (net (code 130) (name "Net-(J1-Pad24)")
      (node (ref J1) (pin 24)))
    (net (code 131) (name "Net-(J1-Pad26)")
      (node (ref J1) (pin 26)))
    (net (code 132) (name "Net-(J1-Pad28)")
      (node (ref J1) (pin 28)))
    (net (code 133) (name "Net-(J1-Pad32)")
      (node (ref J1) (pin 32)))
    (net (code 134) (name "Net-(J1-Pad36)")
      (node (ref J1) (pin 36)))
    (net (code 135) (name "Net-(J1-Pad37)")
      (node (ref J1) (pin 37)))
    (net (code 136) (name "Net-(J1-Pad33)")
      (node (ref J1) (pin 33)))
    (net (code 137) (name "Net-(J1-Pad31)")
      (node (ref J1) (pin 31)))
    (net (code 138) (name "Net-(J1-Pad29)")
      (node (ref J1) (pin 29)))
    (net (code 139) (name "Net-(J1-Pad27)")
      (node (ref J1) (pin 27)))
    (net (code 140) (name "Net-(J1-Pad23)")
      (node (ref J1) (pin 23)))
    (net (code 141) (name "Net-(J1-Pad21)")
      (node (ref J1) (pin 21)))
    (net (code 142) (name "Net-(J1-Pad19)")
      (node (ref J1) (pin 19)))
    (net (code 143) (name "Net-(J1-Pad15)")
      (node (ref J1) (pin 15)))
    (net (code 144) (name "Net-(J1-Pad13)")
      (node (ref J1) (pin 13)))
    (net (code 145) (name "Net-(J1-Pad11)")
      (node (ref J1) (pin 11)))
    (net (code 146) (name "Net-(J1-Pad7)")
      (node (ref J1) (pin 7)))
    (net (code 147) (name "Net-(P7-Pad3)")
      (node (ref R29) (pin 1))
      (node (ref P7) (pin 3)))
    (net (code 148) (name "Net-(P7-Pad4)")
      (node (ref R30) (pin 2))
      (node (ref P7) (pin 4)))
    (net (code 149) (name "Net-(D2-Pad2)")
      (node (ref R17) (pin 1))
      (node (ref D2) (pin 2)))
    (net (code 150) (name "Net-(C41-Pad1)")
      (node (ref U3) (pin 6))
      (node (ref Y1) (pin 2))
      (node (ref C41) (pin 1)))
    (net (code 151) (name "Net-(C40-Pad1)")
      (node (ref U3) (pin 5))
      (node (ref Y1) (pin 1))
      (node (ref C40) (pin 1)))
    (net (code 152) (name "Net-(U3-Pad10)")
      (node (ref U3) (pin 10)))
    (net (code 153) (name "Net-(U3-Pad11)")
      (node (ref U3) (pin 11)))
    (net (code 154) (name "Net-(U3-Pad17)")
      (node (ref U3) (pin 17)))
    (net (code 155) (name "Net-(U3-Pad4)")
      (node (ref U3) (pin 4)))
    (net (code 156) (name "Net-(U3-Pad46)")
      (node (ref U3) (pin 46)))
    (net (code 157) (name "Net-(U3-Pad21)")
      (node (ref U3) (pin 21)))
    (net (code 158) (name "Net-(U3-Pad22)")
      (node (ref U3) (pin 22)))
    (net (code 159) (name "Net-(U3-Pad38)")
      (node (ref U3) (pin 38)))))